**Clock**

* Sources
  + Crystal Oscillator (External to the MCU) (HSE) 8Mhz
  + The RC Oscillator (Internal to the MCU) (HSI)
  + The PLL (Phase Locked Loop) (Internal to the MCU)