**Memory Map of the MCU**

* Arm Cortex M4
* The width of the System Bus is 32bits
* The processor can produce 232 of different addresses. (4G)
* 0x0000\_0000 to 0xffff\_ffff
* When the processor produces 0x4002 0000 on the system bus, it refers to the GPIOA registers.